Leather- Red Hair Sheep Skins- Part3: Guidelines For Grading On the Basis of Mass and Size

WD Stage

Warning

This document is not an ISO International Standard. It is distributed for review and comment. It is subject to change without notice and may not be referred to as an International Standard.

Recipients of this draft are invited to submit, with their comments, notification of any relevant patent rights of which they are aware and to provide supporting documentation.

**Copyright notice**

This ISO document is a working draft or committee draft and is copyright-protected by ISO. While the reproduction of working drafts or committee drafts in any form for use by participants in the ISO standards development process is permitted without prior permission from ISO, neither this document nor any extract from it may be reproduced, stored or transmitted in any form for any other purpose without prior written permission from ISO.

Requests for permission to reproduce this document for the purpose of selling it should be addressed as shown below or to ISO's member body in the country of the requester:

ISO copyright office

Case postale 56 • CH-1211 Geneva 20

Tel. + 41 22 749 01 11

Fax + 41 22 749 09 47

E-mail copyright@iso.org

Web www.iso.org

Reproduction for sales purposes may be subject to royalty payments or a licensing agreement.

Violators may be prosecuted.

ii

Contents

Foreword …………………………………………………………………………………………………………iv

**1 Scope ……………………………………………………………………...............................................................1**

**2 Normative reference ……………………………………………………………………………………………..1**

**3 Terms and definitions ……………………………………………………………………………………………1**

**4 Grading …………………………………………………………………………………………………………...2**

**4.1 Measurement of length and area .......................................................................................................................2**

**4.2 Determination of mass ........................................................................................................................................2**

**4.3 Grading On the basis of size/ mass …………………………………………………………………………...2**

Foreword

ISO (the International Organization for Standardization) is a worldwide federation of national standards bodies (ISO member bodies). The work of preparing International Standards is normally carried out through ISO technical committees. Each member body interested in a subject for which a technical committee has been established has the right to be represented on that committee. International organizations, governmental and non-governmental, in liaison with ISO, also take part in the work. ISO collaborates closely with the International Electrotechnical Commission (IEC) on all matters of electrotechnical standardization.

The procedures used to develop this document and those intended for its further maintenance are described in the ISO/IEC Directives, Part 1. In particular, the different approval criteria needed for the different types of ISO documents should be noted. This document was drafted in accordance with the editorial rules of the ISO/IEC Directives, Part 2 (see www.iso.org/directives ).

ISO draws attention to the possibility that the implementation of this document may involve the use of (a) patent(s).ISO takes no position concerning the evidence, validity or applicability of any claimed patent rights in respect thereof. As of the date of publication of this document, ISO [had/had not] received notice of (a) patent(s) which may be required to implement this document. However, implementers are cautioned that this may not represent the latest information, which may be obtained from the patent database available at www.iso.org/patents . ISO shall not be held responsible for identifying any or all such patent rights.

Any trade name used in this document is information given for the convenience of users and does not constitute an endorsement.

For an explanation of the voluntary nature of standards, the meaning of ISO specific terms and expressions related to conformity assessment, as well as information about ISO&#39;s adherence to the World Trade Organization (WTO) principles in the Technical Barriers to Trade (TBT), see www.iso.org/iso/foreword.html .

ISO 23974‑3 was prepared by Technical Committee ISO/TC 120, *Leather*, Subcommittee SC 1, Raw hides and skins including pickled pelts.

ISO 23974 consists of the following parts, under the general title *Leather — Red Hair Sheep Skin*:

* *Part 1: Description of defects*
* *Part 2: Guidelines for grading on the basis of defects*
* *Part 3: Guidelines for grading on the basis of mass & size*

Any feedback or questions on this document should be directed to the user’s national standards body. A complete listing of these bodies can be found at www.iso.org/members.html .

# Leather – Red Hair Sheep Skins-Part 3: Guidelines For Grading On The Basis Of Mass And Size

# 1 SCOPE

This draft standard prescribes guidelines for grading raw red hair skins on the basis of their mass and size.

**2 NORMATIVE REFERENCES**

There are no norrmative references in this documents.

# 3 TERMS AND DEFINITIONS

For the purpose of this part of standard, the following terms and definitions apply.

**3.1 Butt**

The part of the skin after bellies and shoulders have been removed.

**3.2 Cured skin**

Skin which has been preserved after slaughtering by dry-salting , wet-salting or by sun-drying.

**3.3 Dry salted skin**

Skin dried in air after treating with common salt to preserve for a definite period.

**3.4 Fresh/green skin**

Skin after dissipation of normal body heat, trimmed and defatted and cleaned from dung and extraneous material.

**3.5 Shanks**

That portion of the skin which covers the leg of an animal between the knee and the ankle.

**3.6 Sun-dried skin**

Skin dried under the sun/in air to preserve for a definite period

**3.7 Wet salted skin**

Skin treated with salt to reduce the moisture content for preservation for a definite period.

**4 PRESENTATION**

Red hair sheep skins should be presented in the following forms:

a) Head cut straight behind the ears

b) Shanks cut off at right angles immediately above the knee (fore shanks) and hock (hind shanks)

c) Tail cut off not more than 40 mm from the butt.

**5 GRADING**

**5.1 Grading On the basis of size**

**5.1.1** *Measurement of length and area*

**5.1.1.1** With the skin folded lengthwise along the backbone line and laid flat, the length is measured from the root of the tail to the point where the front part of the throat is widest, measured at right angles to the fold line to the nearest 0.1 dm.

**5.1.1.2** The width of the skin is measured from the midpoint of the backbone line to the end of the belly at right angles to the backbone line to the nearest 0.1 dm.

**5.1.1.3** The area of the skin is determined by multiplying together the length and width measured in accordance with **5.1.1**.1 and **5.1.1.2** and rounding to the nearest 0.1 dm2.

**5.1.2** Red hair sheep skins may be graded either on the basis of the length of the backbone line or on the basis of size (area) in accordance with Table 1.

**TABLE 1**

**Grading of raw red hair sheep skins on the basis of length or size**

|  |  |  |
| --- | --- | --- |
| **Category** | **Length (dm)** | **Size (area) dm2** |
| Extra small | Below 6 | Upto 30 |
| Lamb | 6, 1 to 7 | 31 to 37 |
| Small | 7, 1 to 8 | 38 to 46 |
| Medium | 8, 1 to 9 | 47 to 55 |
| Large | 9, 1 to 10 | 56 to 64 |
| Extra-large | 10, 1 and above | 65 and above |

**5.2 Grading On the basis of Mass**

**5.2.1 Determination of mass**

**5.2.1.1** Both dry salted and wet salted skins should be unfolded and shaken violently by knocking them flesh side down against the floor or on a horse to remove most of the salt. The remaining salt should then be removed by brushing. Skins should then be weighed individually to the nearest 0.1 kg.

**5.2.1.2** Fresh skins should be made free from excess water and weighed to the nearest 0.1 kg.

**5.2.2** Red hair sheep skins may be graded on the basis of mass in accordance withTable 2.

**TABLE 2 – Grading of raw red hair sheep skins on the basis of mass**

|  |  |  |  |
| --- | --- | --- | --- |
| **Category** | **Mass/Kg** | | |
|  | **Wet salted** | **Dry salted** | **Dried** |
| Lights | Upto 0.800 | Upto 0.50 | Upto 0.30 |
| Small | 0.800 to 1.0 | 0.50 to 0.60 | 0.30 to 0.40 |
| Medium | 1.0 to 1.10 | 0.60 to 0.66 | 0.40 to 0.44 |
| Heavy | 1.10 to 1.25 | 0.66 to 0.75 | 0.44 to 0.50 |
| Extra Heavy | 1.25 to 1.50 | 0.75 to 0.90 | 0.50 to 0.60 |

2