**DRAFT AMENDMENT NO. 2**

**TO**

**IS 9436: 2018** **PERFORMANCE REQUIREMENTS AND METHODS OF TEST FOR WHEELS FOR PASSENGER CARS, QUADRICYCLES AND MINI GOODS CARRIERS**

(*First Revision*)

[*Page* 1, *clause* **1**, (*see* also Amendment No. 1)] — Add the following at the end of the clause:

‘This standard is not applicable to the wheels made for vintage cars.’

[*Page* 4, *Table* 2, (*see* also Amendment No. 1)] — Substitute the following NOTE for the existing:

NOTE — For cold formed alumunium 5000 series, magnesium content shall be less than or equal to 3%.

[*Page* 4, *Table* 4, (*see* also Amendment No. 1)] — Substitute the following NOTE for the existing:

NOTE — For cold formed alumunium 5000 series, magnesium content shall be less than or equal to 3%.

[Page 6, Annex B, *Sl No* **8.3** (*see* also Amendment No. 1)] — Substitute the following for the existing:

**‘8.3** Maximum (Front/Rear) Wheel load capacity (kN)’

(TED 07)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Publication Unit, BIS, New Delhi, India