DOC : TXD 23 (21707)

**AMENDMENT NO. 2 JAN 2023**

**TO**

IS 16709 : 2017 TEXTILES — POLYPROPYLENE (PP) WOVEN, LAMINATED, BLOCK BOTTOM VALVE SACKS FOR PACKAGING OF 50 KG

CEMENT— SPECIFICATION

[*Page* 4, *Table* 1, *Sl No*. (x), *Col* 1 to 5] **—** Substitute the following for the existing:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **‘**x) | Air Permeability at 50 mbar, m3/h (*see* Note 4) | As agreed between buyer and seller | ± 6 percent | Annex F’ |

(*Page* 4, *Notes* under *Table* 1) **—** Insert Note 4 after Note 3:

‘**4** Based on the type and grade of cement, blaine surface area of cement, pressure at packer, and packer technology, the resulting air permeability measured in cubic meter per hour at 50 mbar, shall be as agreed to between buyer and seller.’

(TXD 23)