***भारतीय मानक***

***Indian Standard***

 **IS xxxxx : 2024**

 **IEC 62932-1: 2020**

 स्टेशनरी प्रयोग के लिए प्रवाह बैटरी ऊर्जा पद्धति

भाग 1 शब्दावली एवं समान्य पहलू

Flow Battery Energy Systems for Stationary Applications

Part 1 Terminology and General Aspects

ICS 29.220.99

© BIS 2024

© IEC 2020

 

 भारतीय मानक ब्यूरो

BUREAU OF INDIAN STANDARDS

 मानक भवन, 9 बहादुर शाह ज़फर मार्ग, नई दिल्ली - 110002

MANAK BHAVAN, 9 BAHADUR SHAH ZAFAR MARG

NEW DELHI - 110002

 [www.bis.gov.in](http://www.bis.org.in) [www.standardsbis.in](http://www.standardsbis.in)

 **November 2024 Price Group X**

Secondary Cells and Batteries Sectional Committee, ETD 11

NATIONAL FOREWORD

This Indian Standard (Part 1) which is identical withIEC 62932-1: 2020 ‘Flow battery energy systems for stationary applications - Part 1: Terminology and general aspects’ issued by the International Electrotechnical Commission (IEC) was adopted by the Bureau of Indian Standards on the recommendation of Secondary Cells and Batteries Sectional Committee and approval of the Electrotechnical Division Council.

The text of the IEC Standard has been approved as suitable for publication as an Indian Standard without deviations. Certain conventions are, however, not identical to those used in Indian Standards. Attention is particularly drawn to the following:

1. Wherever the words ‘International Standard’ appears referring to this standard, they should be read as ‘Indian Standard’.
2. Comma (,) has been used as a decimal marker, while in Indian Standards the current practice is to use a point (.) as the decimal marker.

Only English language text has been retained while adopting it in this Indian Standard, and as such the page numbers given here are not the same as in the International Standard.

For the purpose of deciding whether a particular requirement of this standard is complied with, the final value, observed or calculated expressing the result of a test, shall be rounded off in accordance with IS 2: 2022 ‘Rules for rounding off numerical values (*second revision*)’. The number of significant places retained in the rounded off value should be the same as that of the specified value in this standard.