**AMENDMENT NO. 1 February 2024**

**TO**

**IS 2553 (Part 3): 2019 SAFETY GLASS – SPECIFICATION PART 3: SOLAR APPLICATIONS**

**(***Page* 1, *clause* **2**) – Insert the following at the end:

|  |  |
| --- | --- |
| ‘5437: 2024 | Rolled Glass — Patterned, Extra Clear Patterned, Wired and Wired - Patterned Glass — Specification ( Second Revision )’ |

**(***Page* 2, *clause* **4.1**) – Substitute the following for the existing:

**‘**For photovoltaic modules, the raw glass shall conform to “extra clear patterned glass” type specified in IS 5437. For solar flat plate collector, the raw glass shall conform to either IS 14900 or “extra clear patterned glass” type specified in IS 5437.**’**