**AMENDMENT No. 1 February 2024**

**TO**

**IS 802 (PART 1 / SECTION 2): 2016 USE OF STRUCTURAL STEEL IN OVERHEAD TRANSMISSION LINE TOWERS – CODE OF PRACTICE**

**PART 1 MATERIALS, LOADS AND DESIGN STRENGTHS**

**Section 2 Design strengths**

(*Fourth Revision*)

[*Page* 4, *clause* **6.3** (a) and (b)] – Substitute the following for the existing:

|  |  |
| --- | --- |
| ‘a) Leg members, ground wire support peak members and lower members of the cross arms in compression | : 120 |
| b) Other members carrying computed stresses  (such as bracings) | : 200’ |

(CED 07)