**AMENDMENT NO. 2 FEBRUARY 2023**

**TO**

**IS 16544 : 2016 ALL GLASS EVACUATED TUBES SOLAR**

**WATER HEATING SYSTEM**

 (*Page* 3, *clause* **6.1.1**) — Substitute ‘kWh/m2’ *for* ‘kW/m2’

[Page 4, Annex A (*see* also Amendment No. 2)] — Add following at the end of note no. 4:

‘**5** The water tank capacity should be mentioned in litres for information.

 **6** The capacity should also be mentioned as kJ/day.’

(*Page* 5, *clause* **D-1**) — Substitute ‘*H* > 4.7 kWh/m2.d’ *for* ‘*H* > 17 MJ/(m2.d)’

(MED 04)