**AMENDMENT NO. 1 DECEMBER 2024**

**TO**

**IS 17077 (Part 2) : 2020 PLASTICS — ACRYLONITRILE-BUTADIENE-STYRENE**

**(ABS) MOULDING AND EXTRUSION MATERIALS**

**PART 2 PREPARATION OF TEST SPECIMENS AND DETERMINATION OF PROPERTIES**

[*Page* 5, *Table* 3, Vicat softening temperature, *col* (6)] — Substitute ‘50 K/h’ *for* ‘50 ºC/h’.

(PCD 12)