AMENDMENT NO. 3 SEPTEMBER 2024

TO

IS 16490: 2016 LED DESTINATION BOARD SYSTEM FOR BUSES — SPECIFICATION

[*Page* 2, *clause* **A-1.4** (f), *Amendment* 2] ― Substitute the following for the existing:

‘Inner sign should be able to display text and customized graphics and announce up to 9 pre- recorded messages (including those for public awareness like road safety etc.) by driver selecting 1~9 on display panel of the ‘Controller’. This requirement applies only for LDBS Controller types as defined in **4.3.1** (d);’

[*Page* 3, *clause* **A-1.5**, *Para* 1, *Amendment* 2] ― Substitute the following for the existing:

‘**A-1.5** Two-way communication with central control centre via LDBS controller: The requirements mentioned below apply only for LDBS controller types as defined in **4.3.1**(c) and **4.3.1**(d).’

(TED 28)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Publication Unit, BIS, New Delhi, India