***भारतीय मानक***

***Indian Standard***

 **IS XXXX : 2024**

 **ISO 23480 : 2013**

 **दबाने के उपकरण — स्लाइडिंग *प्लेट***

**Tools for Pressing — Sliding Plates**

 ICS 25.120.10

© BIS 2024

© ISO 2013



भारतीय मानक ब्यूरो

BUREAU OF INDIAN STANDARDS

मानक भवन, 9 बहादुर शाह ज़फर मार्ग, नई दिल्ली - 110002

MANAK BHAVAN, 9 BAHADUR SHAH ZAFAR MARG

NEW DELHI - 110002

[www.bis.gov.in](http://www.bis.org.in) [www.standardsbis.in](http://www.standardsbis.in)

**December 2024 Price Group X**

Metal Forming Machines Sectional Committee, PGD 04

NATIONAL FOREWORD

This Indian Standard which is identical with ISO 23480 : 2013 ‘Tools for Pressing — Sliding Plates’ issued by the International Organization for Standardization (ISO) was adopted by the Bureau of Indian Standards on the recommendation of the Metal Forming Machines Sectional Committee and approval of the Production and General Engineering Division Council.

This Standard specifies the main dimensions and tolerances of sliding plates, to be used in press tools. It also specifies the designation of sliding plates.

The text of ISO Standard has been approved as suitable for publication as an Indian Standard without deviations. Certain conventions are, however, not identical to those used in Indian Standards. Attention is particularly drawn to the following:

a) Wherever the words ‘International Standard’ appear referring to this standard, they should be read as ‘Indian Standard’.

b) Comma (,) has been used as a decimal marker while in Indian Standards, the current practice is to use a point (.) as the decimal marker.

In this adopted standard, reference appears to certain International Standards for which Indian Standards also exist. The corresponding Indian Standards, which are to be substituted in their respective places, are listed below along with their degree of equivalence for the editions indicated:

|  |  |  |
| --- | --- | --- |
| *International Standard* | *Corresponding Indian Standard* | *Degree of Equivalence* |
| ISO 2768-1 : 1989 General tolerances — Part 1: Tolerances for linear and angular dimensions without individual tolerance indications | IS 2102 (Part 1) : 1993/ ISO 2768-1 : 1989 General tolerances: Part 1 Tolerances for linear and angular dimensions without individual tolerance indications (*third revision*) | *Identical* |
| ISO 4762 : 2004 Hexagon socket head cap screws  | IS 2269 : 2006/ ISO 4762 : 2004 Hexagon socket head cap screws (*fifth revision*) | *Identical* |

The standard also makes a reference to the BIS Certification Marking of the product. Details of which are given in National Annex A.

For the purpose of deciding whether a particular requirement of this standard is complied with, the final value, observed or calculated expressing the result of a test or analysis, shall be rounded off in accordance with IS 2 : 2022 ‘Rules for rounding off numerical values (*second revision*)’.

**NATIONAL ANNEX A**

(*National Foreword*)

**A-1 BIS CERTIFICATION MARKING**

The product(s) conforming to the requirements of this standard may be certified as per the conformity assessment schemes under the provisions of the *Bureau of Indian Standards Act,* 2016 and the Rules and Regulations framed thereunder, and the products may be marked with the standard mark.